Name : \_\_\_\_\_\_\_\_\_\_\_\_\_

Date : \_\_\_\_\_\_\_\_\_\_\_\_\_

1) The first compliance date of GHS?

a) December 1, 2013

b) January 15, 2014

c) December 31, 2020

d) March 15, 2015

2) \_\_\_\_\_\_\_\_ is used to indicate the relative level of severity of hazard and alert the reader to a potential hazard on the label. There are only two signal words, “Danger” and “Warning”

a) Label Word

b) Signal word

c) Warning Title

d) Danger Zone

3) Product identifier is how the hazardous chemical is identified. This can be by their?

a) Chemical name

b) Product number

c) Trade name

d) All of the Above

4) What is GHS?

a) Globe Hazards System

b) Globally Harmonized System for Hazard Classification & Labeling

c) Green Hazard Signs

d) None of the Above

5) Which signal word on a label represents the more severe hazard?

a) Danger

b) Warning

6) Under the hazcom standards your employer must inform you of ways to protect yourself from hazardous chemicals by using safe work practices, emergency procedures and Personal Protective Equipment.

a) True

b) False

7) Under OSHA’s GHS Rule MSDS’s will be replaced with SDS’s Safety Data Sheets.

a) True

b) False

8) Hazard statement describes the nature of the hazard(s) of a chemical, including one or more hazards on each label?

a) True

b) False

9) Precautionary statement means a phrase that describes recommended measures that should be taken to minimize or prevent adverse effects resulting from exposure to a hazardous chemical or improper storage or handling?

a) True

b) False

10) Safety Data Sheets provide instructions for safely handling and storing material.

a) True

b) False

11) Health hazards can include symptoms such as stomach aches, nausea, and reproductive damage.

a) True

b) False

12) Acute health hazards occur gradually over time.

a) True

b) False

13) There are 114 Hazard statements overall and 140 Precautionary statements that could be found on a label.

a) True

b) False

14) GHS training is required annually.

a) True

b) False

15) OSHA’s required pictograms must be in the shape of a square set at a point and include a black hazard symbol on a white background with a red frame sufficiently wide enough to be clearly visible.

a) True

b) False

16) CFD Hazard Communications Operating Procedure can be found where?

a) In CFD Operating Procedure Book

b) In the Hazcom SDS Book located in the Hazcom Station.

c) a and b